{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Principal"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Principal","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[[15,1,15,2],[15,5,16,9],[16,1,16,2],[17,1,17,2],[12,5,12,6],[14,5,14,6],[1,2,3,7],[6,1,6,3],[10,1,10,2],[11,1,11,2],[6,5,6,7],[10,5,10,6],[14,1,14,2]]}
[]
[null,null,"Ferraillage des murs voiles et justifications selon RPA2024"]
[]
[]
[null,null,null,"abdellatif-megnounif.com",null,"Mes cours\\RPA2024"]
[]
[null,"Données de la structure",null,null,null,"Données Matériaux"]
[null,"Longueur du mur (m) lw=",null,null,null,"Contrainte béton Fc28 (Mpa)"]
[null,"Epaisseur du mur (m) bw=",null,null,null,"Contrainte acier Fe (Mpa)"]
[null,"Hauteur totale du mur (m) hw=",null,null,null,"Coefficient béton Gamab"]
[null,"Hauteur libre d'étages (m) he=",null,null,null,"Coefficient Acier GamaS"]
[null,"Nombre d'étages"]
[null,"Facteur de qualité Qf",null,null,null,"Moment résistant MRd (KN.m)"]
[null,"Période propre T0 (s)"]
[null,"Période T2 (s)"]
[null,"Zone sismique",null,null,null,"REM : Commencer par remplir les donnees dans les cellules vertes, puis appuyer sur Verification. "]
[null,"Type de contreventement"]
[null,"Type de Voile"]